Speed Passion Reventon PC Interface Safe Mode user guide

1. Open Reventon PC Interface
2. Click Key “S”,  a pop-up dialog “You entered safe mode” display and  “Safe mode” label display on the top right hand corner
3. Connect Reventon LCD Program Card to PC by pressing the “Value” button
4. Connect Reventon ESC to LCD Program Card
5. A popup dialog “Connect ESC” show and press “No”
6. An “update firmware” button will show on the left hand side. 
7. Click on “update firmware” button and then “select  firmware” dialog shown
8. Choose the corresponding firmware and press “Ok” button
9. A confirm dialog will pop-up and press “Yes” button to continue
10. update firmware process will start.
11. Once the update process success, the PC Interface will return to “home screen” and exit safe mode